
**How to upgrade firmware of Wireless Extender for USB Cameras**

1. Please check whether your computer's Wi-Fi connection is turned on and enable an internet connection. Then power the EXW01-TX and connect EXW01-RX to your computer.


2. Start the " Firmware Upgrade Tool". If the latest firmware is available for download on the internet, the tool will download the latest firmware.









3. Click "START SEARCHING" to find device.



4. After finishing the search, you should see the devices listed as “WUVCTX-xxxxxx” and “WUVCRX-xxxxxx”.

**Please select “WUVCRX-xxxxxx” or “WUVCTX-xxxxxx” to connect to.**






5. After connecting to the device, the dialog box will show the firmware information. Now you can click the Update Firmware button to upgrade the device firmware.

**Notes: DO NOT turn off the power during the upgrade process, otherwise it may cause permanent damage to the product.**





6. After the upgrade process is completed, press OK to continue. wait for some time for the system to restart.



